(footprint "DSG0008A_TEX" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tags "TPS61021ADSGR ")
  (attr smd)
  (fp_text reference "REF**" (at 0 0 unlocked) (layer F.SilkS))
  (fp_text value DSG0008A_TEX (at 0 0 unlocked) (layer F.Fab))
  (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer F.Fab))
  (pad "1" smd roundrect (at -0.950001 -0.750001) (size 0.508 0.254) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd roundrect (at -0.950001 -0.25) (size 0.508 0.254) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "3" smd roundrect (at -0.950001 0.25) (size 0.508 0.254) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "4" smd roundrect (at -0.950001 0.750001) (size 0.508 0.254) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "5" smd roundrect (at 0.950001 0.750001) (size 0.508 0.254) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "6" smd roundrect (at 0.950001 0.25) (size 0.508 0.254) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "7" smd roundrect (at 0.950001 -0.25) (size 0.508 0.254) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "8" smd roundrect (at 0.950001 -0.750001) (size 0.508 0.254) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "9" smd rect (at 0 0) (size 0.889 1.6002) (layers "F.Cu"))
)
