(footprint "DWM1000"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "IEEE802.15.4-2011 UWB")
	(tags "UWB Module")
	(property "Reference" "REF**"
		(at -5.08 13.97 0)
		(layer "F.SilkS")
	)
	(property "Value" "DWM1000"
		(at 0 7.5 0)
		(layer "F.Fab")
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "KEEP-OUT ZONE"
		(at 0 -8.89 0)
		(layer "Cmts.User")
	)
	(fp_text user "no components, traces, or copper on any layer"
		(at 0 -6.35 0)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -6.3 -0.7988 90)
		(size 1 2.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "2" smd rect
		(at -6.3 0.6012 90)
		(size 1 2.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "3" smd rect
		(at -6.3 2.0012 90)
		(size 1 2.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "4" smd rect
		(at -6.3 3.4012 90)
		(size 1 2.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "5" smd rect
		(at -6.3 4.8012 90)
		(size 1 2.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "6" smd rect
		(at -6.3 6.2012 90)
		(size 1 2.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "7" smd rect
		(at -6.3 7.6012 90)
		(size 1 2.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "8" smd rect
		(at -6.3 9.0012 90)
		(size 1 2.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "9" smd rect
		(at -4.9 11.2962)
		(size 1 2.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "10" smd rect
		(at -3.5 11.2962)
		(size 1 2.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "11" smd rect
		(at -2.1 11.2962)
		(size 1 2.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "12" smd rect
		(at -0.7 11.2962)
		(size 1 2.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "13" smd rect
		(at 0.7 11.2962)
		(size 1 2.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "14" smd rect
		(at 2.1 11.2962)
		(size 1 2.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "15" smd rect
		(at 3.5 11.2962)
		(size 1 2.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "16" smd rect
		(at 4.9 11.2962)
		(size 1 2.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "17" smd rect
		(at 6.3 9 90)
		(size 1 2.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "18" smd rect
		(at 6.3 7.6 90)
		(size 1 2.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "19" smd rect
		(at 6.3 6.2012 90)
		(size 1 2.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "20" smd rect
		(at 6.3 4.8012 90)
		(size 1 2.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "21" smd rect
		(at 6.3 3.4012 90)
		(size 1 2.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "22" smd rect
		(at 6.3 2.0012 90)
		(size 1 2.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "23" smd rect
		(at 6.3 0.6012 90)
		(size 1 2.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "24" smd rect
		(at 6.3 -0.7988 90)
		(size 1 2.45)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(zone
		(net 0)
		(net_name "")
		(layers "*.Cu")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -8.89 -1.32) (xy 8.89 -1.32) (xy 8.89 -12.7) (xy -8.89 -12.7)
			)
		)
	)
	(model "${KICAD8_3DMODEL_DIR}/RF_Module.3dshapes/DWM1000.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)