(module Diode_THT:D_DO-201AD_P5.08mm_Vertical_AnodeUp (layer F.Cu) (tedit 5AE50CD5)
  (descr "Diode, DO-201AD series, Axial, Vertical, pin pitch=5.08mm, , length*diameter=9.5*5.2mm^2, , http://www.diodes.com/_files/packages/DO-201AD.pdf")
  (tags "Diode DO-201AD series Axial Vertical pin pitch 5.08mm  length 9.5mm diameter 5.2mm")
  (fp_text reference REF** (at 2.54 -3.72) (layer F.SilkS))
  (fp_text value D_DO-201AD_P5.08mm_Vertical_AnodeUp (at 2.54 5.498) (layer F.Fab))
  (fp_text user A (at 5.08 2.6) (layer F.SilkS))
  (fp_text user A (at 5.08 2.6) (layer F.Fab))
  (fp_text user %R (at 2.54 -3.72) (layer F.Fab))
  (pad 2 thru_hole oval (at 5.08 0) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask))
  (pad 1 thru_hole rect (at 0 0) (size 3.2 3.2) (drill 1.6) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Diode_THT.3dshapes/D_DO-201AD_P5.08mm_Vertical_AnodeUp.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
