(module Diode_SMD:Diode_Bridge_Diotec_ABS (layer F.Cu) (tedit 5A4F6D53)
  (descr "SMD diode bridge ABS (Diotec), see https://diotec.com/tl_files/diotec/files/pdf/datasheets/abs2.pdf")
  (tags "ABS MBLS")
  (attr smd)
  (fp_text reference REF** (at 0 -3.7) (layer F.SilkS))
  (fp_text value Diode_Bridge_Diotec_ABS (at 0 3.7) (layer F.Fab))
  (fp_text user %R (at 0 -0.065) (layer F.Fab))
  (pad 4 smd rect (at 2.975 -2) (size 1 0.7) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 2.975 2) (size 1 0.7) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -2.975 2) (size 1 0.7) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -2.975 -2) (size 1 0.7) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/Diode_SMD.3dshapes/Diode_Bridge_Diotec_ABS.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
