(module Diode_THT:Diode_Bridge_Round_D9.8mm (layer F.Cu) (tedit 5A142105)
  (descr "4-lead round diode bridge package, diameter 9.8mm, pin pitch 5.08mm, see http://www.vishay.com/docs/88769/woo5g.pdf")
  (tags "diode bridge 9.8mm WOG pitch 5.08mm")
  (fp_text reference REF** (at 2.54 -3.302) (layer F.SilkS))
  (fp_text value Diode_Bridge_Round_D9.8mm (at 2.6035 8.509) (layer F.Fab))
  (fp_text user %R (at 3.81 2.54) (layer F.Fab))
  (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  (pad 3 thru_hole oval (at 5.08 5.08) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 0 5.08) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  (pad 4 thru_hole oval (at 5.08 0) (size 2 2) (drill 1) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Diode_THT.3dshapes/Diode_Bridge_Round_D9.8mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
