(footprint "Diodes_UDFN-10_1.0x2.5mm_P0.5mm"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "U-DFN2510-10 package used by Diodes Incorporated (https://www.diodes.com/assets/Package-Files/U-DFN2510-10-Type-CJ.pdf)")
	(tags "UDFN-10 U-DFN2510-10 Diodes")
	(property "Reference" "REF**"
		(at 0 -2.54 0)
		(layer "F.SilkS")
	)
	(property "Value" "Diodes_UDFN-10_1.0x2.5mm_P0.5mm"
		(at 0 2.54 0)
		(layer "F.Fab")
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 90)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -0.3875 -1 270)
		(size 0.25 0.625)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "2" smd rect
		(at -0.3875 -0.5 270)
		(size 0.25 0.625)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "3" smd rect
		(at -0.35 0 270)
		(size 0.45 0.7)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "4" smd rect
		(at -0.3875 0.5 270)
		(size 0.25 0.625)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "5" smd rect
		(at -0.3875 1 270)
		(size 0.25 0.625)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "6" smd rect
		(at 0.3875 1 270)
		(size 0.25 0.625)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "7" smd rect
		(at 0.3875 0.5 270)
		(size 0.25 0.625)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "8" smd rect
		(at 0.4125 0 270)
		(size 0.45 0.575)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "9" smd rect
		(at 0.3875 -0.5 270)
		(size 0.25 0.625)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "10" smd rect
		(at 0.3875 -1 270)
		(size 0.25 0.625)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(model "${KICAD8_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/Diodes_UDFN-10_1.0x2.5mm_P0.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)