(footprint "DirectFET_MX"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "DirectFET MX https://www.infineon.com/dgdl/Infineon-AN-1035-ApplicationNotes-v29_01-EN.pdf?fileId=5546d462533600a40153559159020f76#page=27")
	(tags "DirectFET MX MOSFET Infineon")
	(property "Reference" "REF**"
		(at 0 -3.5 0)
		(layer "F.SilkS")
	)
	(property "Value" "DirectFET_MX"
		(at 0 3.5 0)
		(layer "F.Fab")
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -3.2 -1.175)
		(size 0.9 1.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1" smd rect
		(at -3.2 1.175)
		(size 0.9 1.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1" smd rect
		(at 3.2 -1.175)
		(size 0.9 1.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "1" smd rect
		(at 3.2 1.175)
		(size 0.9 1.85)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "2" smd rect
		(at -1.45 0)
		(size 0.75 0.75)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "3" smd rect
		(at 0.3 -0.61)
		(size 1.45 0.87)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "3" smd rect
		(at 0.3 0.61)
		(size 1.45 0.87)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(model "${KICAD8_3DMODEL_DIR}/Package_DirectFET.3dshapes/DirectFET_MX.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)