(module EPC2045 (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value EPC2045 (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.2in/5.08mm" (at -3.663 0) (layer Cmts.User))
  (fp_text user "0.15in/3.81mm" (at 0 3.163) (layer Cmts.User))
  (fp_text user "0.02in/0.5mm" (at 3.663 -0.25) (layer Cmts.User))
  (fp_text user "0.013in/0.32mm" (at 3.663 0.5) (layer Cmts.User))
  (pad 1 smd circle (at -1 -0.45) (size 0.319989 0.319989) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd circle (at -0.5 -0.45) (size 0.319989 0.319989) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd circle (at 0 -0.45) (size 0.319989 0.319989) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd circle (at 0.5 -0.45) (size 0.319989 0.319989) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd circle (at 1 -0.45) (size 0.319989 0.319989) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd circle (at -1 0) (size 0.319989 0.319989) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd circle (at -0.5 0) (size 0.319989 0.319989) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd circle (at 0 0) (size 0.319989 0.319989) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd circle (at 0.5 0) (size 0.319989 0.319989) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd circle (at 1 0) (size 0.319989 0.319989) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd circle (at -1 0.45) (size 0.319989 0.319989) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd circle (at -0.5 0.45) (size 0.319989 0.319989) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd circle (at 0 0.45) (size 0.319989 0.319989) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd circle (at 0.5 0.45) (size 0.319989 0.319989) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd circle (at 1 0.45) (size 0.319989 0.319989) (layers F.Cu F.Paste F.Mask))
)
