(module EPC2111 (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value EPC2111_ECC (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "" (at 1.397 -1.5) (layer F.SilkS))
  (fp_text user "" (at 1.397 -1.5) (layer F.Fab))
  (fp_text user "" (at 1.397 -1.5) (layer B.SilkS))
  (fp_text user "" (at 1.397 1.5) (layer F.SilkS))
  (fp_text user "" (at 1.397 1.5) (layer F.Fab))
  (fp_text user "" (at 1.397 1.5) (layer B.SilkS))
  (fp_text user "3" (at -0.5 -2.4003 90) (layer F.SilkS))
  (fp_text user "3" (at -0.5 -2.4003 90) (layer F.Fab))
  (fp_text user "3" (at -0.5 -2.4003 90) (layer B.SilkS))
  (fp_text user "1" (at 0.5 -2.4003 90) (layer F.SilkS))
  (fp_text user "1" (at 0.5 -2.4003 90) (layer F.Fab))
  (fp_text user "1" (at 0.5 -2.4003 90) (layer B.SilkS))
  (fp_text user "0.2in/5.08mm" (at -3.175 0) (layer Cmts.User))
  (fp_text user "0.15in/3.81mm" (at 0 4.1783) (layer Cmts.User))
  (fp_text user "0.02in/0.5mm" (at 3.175 -1.25) (layer Cmts.User))
  (fp_text user "0.009in/0.229mm" (at 3.175 1.5) (layer Cmts.User))
  (pad 3 smd circle (at -0.5 -1.5) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd circle (at 0 -1.5) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd circle (at 0.5 -1.5) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd circle (at -0.5 -1) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd circle (at 0 -1) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd circle (at 0.5 -1) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd circle (at -0.5 -0.5) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd circle (at 0 -0.5) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd circle (at 0.5 -0.5) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd circle (at -0.5 0) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd circle (at 0 0) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd circle (at 0.5 0) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd circle (at -0.5 0.5) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd circle (at 0 0.5) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd circle (at 0.5 0.5) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (pad 18 smd circle (at -0.5 1) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (pad 17 smd circle (at 0 1) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd circle (at 0.5 1) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (pad 21 smd circle (at -0.5 1.5) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (pad 20 smd circle (at 0 1.5) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (pad 19 smd circle (at 0.5 1.5) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
)
