(module EPC2216 (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value EPC2216_ECC (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "1" (at -1.0541 -0.4) (layer F.SilkS))
  (fp_text user "1" (at -1.0541 -0.4) (layer F.Fab))
  (fp_text user "1" (at -1.0541 -0.4) (layer B.SilkS))
  (fp_text user "3" (at -1.0541 0.4) (layer F.SilkS))
  (fp_text user "3" (at -1.0541 0.4) (layer F.Fab))
  (fp_text user "3" (at -1.0541 0.4) (layer B.SilkS))
  (fp_text user "" (at -0.2 -1.2319 90) (layer F.SilkS))
  (fp_text user "" (at -0.2 -1.2319 90) (layer F.Fab))
  (fp_text user "" (at -0.2 -1.2319 90) (layer B.SilkS))
  (fp_text user "" (at 0.2 -1.2319 90) (layer F.SilkS))
  (fp_text user "" (at 0.2 -1.2319 90) (layer F.Fab))
  (fp_text user "" (at 0.2 -1.2319 90) (layer B.SilkS))
  (fp_text user "0.016in/0.4mm" (at 2.8321 -0.2) (layer Cmts.User))
  (fp_text user "0.009in/0.229mm" (at 2.8321 0.4) (layer Cmts.User))
  (pad 1 smd circle (at -0.2 -0.4) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd circle (at 0.2 -0.4) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd circle (at -0.2 0) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd circle (at 0.2 0) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd circle (at -0.2 0.4) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd circle (at 0.2 0.4) (size 0.2286 0.2286) (layers F.Cu F.Paste F.Mask))
)
