(module ESDZL5-1F4 (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value CR_ESDZL5-1F4_STM (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.01in/0.254mm" (at 3.2131 0) (layer Cmts.User))
  (fp_text user "0.008in/0.203mm" (at -0.1651 1.9304) (layer Cmts.User))
  (pad 1 smd rect (at -0.1651 0) (size 0.2032 0.254) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 0.1651 0) (size 0.2032 0.254) (layers F.Cu F.Paste F.Mask))
)
