(footprint "ESP32-WROOM-32"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Single 2.4 GHz Wi-Fi and Bluetooth combo chip https://www.espressif.com/sites/default/files/documentation/esp32-wroom-32_datasheet_en.pdf")
	(tags "Single 2.4 GHz Wi-Fi and Bluetooth combo  chip")
	(property "Reference" "REF**"
		(at -10.61 8.43 90)
		(layer "F.SilkS")
	)
	(property "Value" "ESP32-WROOM-32"
		(at 0 11.5 0)
		(layer "F.Fab")
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "KEEP-OUT ZONE"
		(at 0.05 -22.48 0)
		(layer "Cmts.User")
	)
	(fp_text user "Antenna"
		(at 0 -13 0)
		(layer "Cmts.User")
	)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -8.75 -8.25)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "2" smd rect
		(at -8.75 -6.98)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "3" smd rect
		(at -8.75 -5.71)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "4" smd rect
		(at -8.75 -4.44)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "5" smd rect
		(at -8.75 -3.17)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "6" smd rect
		(at -8.75 -1.9)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "7" smd rect
		(at -8.75 -0.63)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "8" smd rect
		(at -8.75 0.64)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "9" smd rect
		(at -8.75 1.91)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "10" smd rect
		(at -8.75 3.18)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "11" smd rect
		(at -8.75 4.45)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "12" smd rect
		(at -8.75 5.72)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "13" smd rect
		(at -8.75 6.99)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "14" smd rect
		(at -8.75 8.26)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "15" smd rect
		(at -5.71 9.51 90)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "16" smd rect
		(at -4.44 9.51 90)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "17" smd rect
		(at -3.17 9.51 90)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "18" smd rect
		(at -1.9 9.51 90)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "19" smd rect
		(at -0.63 9.51 90)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "20" smd rect
		(at 0.64 9.51 90)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "21" smd rect
		(at 1.91 9.51 90)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "22" smd rect
		(at 3.18 9.51 90)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "23" smd rect
		(at 4.45 9.51 90)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "24" smd rect
		(at 5.72 9.51 90)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "25" smd rect
		(at 8.75 8.26)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "26" smd rect
		(at 8.75 6.99)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "27" smd rect
		(at 8.75 5.72)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "28" smd rect
		(at 8.75 4.45)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "29" smd rect
		(at 8.75 3.18)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "30" smd rect
		(at 8.75 1.91)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "31" smd rect
		(at 8.75 0.64)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "32" smd rect
		(at 8.75 -0.63)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "33" smd rect
		(at 8.75 -1.9)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "34" smd rect
		(at 8.75 -3.17)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "35" smd rect
		(at 8.75 -4.44)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "36" smd rect
		(at 8.75 -5.71)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "37" smd rect
		(at 8.75 -6.98)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "38" smd rect
		(at 8.75 -8.25)
		(size 1.5 0.9)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "39" smd rect
		(at -2.205 -2.435)
		(size 1.05 1.05)
		(layers "F.Cu" "F.Paste")
	)
	(pad "39" thru_hole circle
		(at -2.205 -1.6725)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "39" smd rect
		(at -2.205 -0.91)
		(size 1.05 1.05)
		(layers "F.Cu" "F.Paste")
	)
	(pad "39" thru_hole circle
		(at -2.205 -0.1475)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "39" smd rect
		(at -2.205 0.615)
		(size 1.05 1.05)
		(layers "F.Cu" "F.Paste")
	)
	(pad "39" thru_hole circle
		(at -1.4425 -2.435)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "39" thru_hole circle
		(at -1.4425 -0.91)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "39" thru_hole circle
		(at -1.4425 0.615)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "39" smd rect
		(at -0.68 -2.435)
		(size 1.05 1.05)
		(layers "F.Cu" "F.Paste")
	)
	(pad "39" thru_hole circle
		(at -0.68 -1.6725)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "39" smd rect
		(at -0.68 -0.91)
		(size 1.05 1.05)
		(layers "F.Cu" "F.Paste")
	)
	(pad "39" smd rect
		(at -0.68 -0.91)
		(size 4.2 4.2)
		(layers "F.Cu" "F.Mask")
	)
	(pad "39" thru_hole circle
		(at -0.68 -0.1475)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "39" smd rect
		(at -0.68 0.615)
		(size 1.05 1.05)
		(layers "F.Cu" "F.Paste")
	)
	(pad "39" thru_hole circle
		(at 0.0825 -2.435)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "39" thru_hole circle
		(at 0.0825 -0.91)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "39" thru_hole circle
		(at 0.0825 0.615)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "39" smd rect
		(at 0.845 -2.435)
		(size 1.05 1.05)
		(layers "F.Cu" "F.Paste")
	)
	(pad "39" thru_hole circle
		(at 0.845 -1.6725)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "39" smd rect
		(at 0.845 -0.91)
		(size 1.05 1.05)
		(layers "F.Cu" "F.Paste")
	)
	(pad "39" thru_hole circle
		(at 0.845 -0.1475)
		(size 0.6 0.6)
		(drill 0.2)
		(property pad_prop_heatsink)
		(layers "*.Cu" "F.Mask")
		(remove_unused_layers no)
	)
	(pad "39" smd rect
		(at 0.845 0.615)
		(size 1.05 1.05)
		(layers "F.Cu" "F.Paste")
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "In1.Cu" "B.Cu")
		(hatch full 0.508)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.254)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints not_allowed)
		)
		(fill
			(thermal_gap 0.508)
			(thermal_bridge_width 0.508)
		)
		(polygon
			(pts
				(xy -24 -9.8) (xy 24 -9.8) (xy 24 -30.74) (xy -24 -30.74)
			)
		)
	)
	(model "${KICAD8_3DMODEL_DIR}/RF_Module.3dshapes/ESP32-WROOM-32.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)