(module EXB34V331JV (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value C_ARRAY_EXB34V_PAN (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "*" (at -0.4953 -0.3937) (layer F.Fab))
  (fp_text user "*" (at -1.2573 -1.6129) (layer F.SilkS))
  (pad 1 smd rect (at -0.889 -0.8255) (size 0.889 1.0668) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -0.889 0.8255) (size 0.889 1.0668) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 0.889 0.8255) (size 0.889 1.0668) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 0.889 -0.8255) (size 0.889 1.0668) (layers F.Cu F.Paste F.Mask))
)
