(module EXBA10P121J (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value C_ARRAY_EXBA_PAN (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "*" (at -1.016 -2.794) (layer F.Fab))
  (fp_text user "*" (at -2.286 -3.4036) (layer F.SilkS))
  (pad 1 smd rect (at -1.7399 -2.54) (size 0.7366 0.6096) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.7399 -1.27) (size 0.7366 0.6096) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -1.7399 0) (size 0.7366 0.6096) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -1.7399 1.27) (size 0.7366 0.6096) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -1.7399 2.54) (size 0.7366 0.6096) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 1.7399 2.54) (size 0.7366 0.6096) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 1.7399 1.27) (size 0.7366 0.6096) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 1.7399 0) (size 0.7366 0.6096) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 1.7399 -1.27) (size 0.7366 0.6096) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at 1.7399 -2.54) (size 0.7366 0.6096) (layers F.Cu F.Paste F.Mask))
)
