(module Everlight_ITR8307 (layer F.Cu) (tedit 5B870839)
  (descr "package for Everlight ITR8307 with PCB cutout, light-direction upwards, see http://www.everlight.com/file/ProductFile/ITR8307.pdf")
  (tags "refective opto couple photo coupler")
  (attr smd)
  (fp_text reference REF** (at -2.8 0 90) (layer F.SilkS))
  (fp_text value Everlight_ITR8307 (at 0 4.8) (layer F.Fab))
  (fp_text user %R (at 0 0.2) (layer F.Fab))
  (fp_line (start 1.85 1.8) (end -1.85 1.8) (layer Edge.Cuts) (width 0.12))
  (fp_line (start 1.85 -1.8) (end 1.85 1.8) (layer Edge.Cuts) (width 0.12))
  (fp_line (start -1.85 -1.8) (end 1.85 -1.8) (layer Edge.Cuts) (width 0.12))
  (fp_line (start -1.85 1.8) (end -1.85 -1.8) (layer Edge.Cuts) (width 0.12))
  (pad 3 smd rect (at 0.9 2.8) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2))
  (pad 1 smd rect (at -0.9 2.8) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2))
  (pad 2 smd rect (at -0.9 -2.8) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2))
  (pad 4 smd rect (at 0.9 -2.8) (size 1.2 1.4) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2))
  (model ${KISYS3DMOD}/OptoDevice.3dshapes/Everlight_ITR8307.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
