(module FA-128 32.0000MF10Z-AJ3 (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value FA-128_EPS (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.038in/0.952mm" (at -1.778 0.9525) (layer Cmts.User))
  (fp_text user "0.024in/0.61mm" (at 0.3048 -3.6703) (layer Cmts.User))
  (fp_text user "0.02in/0.508mm" (at -2.7432 0.6223) (layer Cmts.User))
  (fp_text user "-0.024in/-0.61mm" (at 0 6.2103) (layer Cmts.User))
  (fp_text user "0.049in/1.245mm" (at 5.2832 0.635) (layer Cmts.User))
  (fp_text user "*" (at -0.47625 -1.5621) (layer F.SilkS))
  (fp_text user "*" (at -0.47625 -0.3175) (layer F.Fab))
  (pad 1 smd rect (at -0.47625 -0.6223) (size 0.508 0.6096) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -0.47625 0.6223) (size 0.508 0.6096) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 0.47625 0.6223) (size 0.508 0.6096) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 0.47625 -0.6223) (size 0.508 0.6096) (layers F.Cu F.Paste F.Mask))
)
