(footprint "FC0V474ZFTBR24_KEM" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tags "FC0V474ZFTBR24 ")
  (attr smd)
  (fp_text reference "REF**" (at 0 0 unlocked) (layer F.SilkS))
  (fp_text value FC0V474ZFTBR24_KEM (at 0 0 unlocked) (layer F.Fab))
  (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer F.Fab))
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -2.5654 -0.9017)
        (xy 2.5654 -0.9017)
        (xy 2.5654 0.9017)
        (xy -2.5654 0.9017)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -5.3467 -5.3467)
        (xy 5.3467 -5.3467)
        (xy 5.3467 -0.9017)
        (xy -5.3467 -0.9017)
      )
    )
  )
  (zone (net 0) (net_name "") (layer "F.Cu") (hatch full 0.508)
    (connect_pads (clearance 0))
    (min_thickness 0.254)
    (keepout (tracks not_allowed) (vias not_allowed) (pads allowed ) (copperpour not_allowed) (footprints allowed))
    (fill (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy -5.3467 0.9017)
        (xy 5.3467 0.9017)
        (xy 5.3467 5.3467)
        (xy -5.3467 5.3467)
      )
    )
  )
  (pad "1" smd rect (at -4.8641 0) (size 4.4958 1.7018) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at 4.8641 0) (size 4.4958 1.7018) (layers "F.Cu" "F.Paste" "F.Mask"))
)
