(module FCR7350R (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value CONN1_FCR7350R_CLF (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (pad 1 thru_hole circle (at 0 0) (size 2.7178 2.7178) (drill 2.2098) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at -5.08 -3.8 90) (size 1.7018 1.7018) (drill 1.1938) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 5.08 -3.8 90) (size 1.7018 1.7018) (drill 1.1938) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at -5.08 6.36 90) (size 1.7018 1.7018) (drill 1.1938) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 5.08 6.36 90) (size 1.7018 1.7018) (drill 1.1938) (layers *.Cu *.Mask))
)
