(module Connector_PinHeader_2.54mm:PinHeader_1x08_P2.54mm_Vertical (layer F.Cu) (tedit 656C88E9)
  (descr "Through hole straight pin header, 1x08, 2.54mm pitch, single row")
  (tags "Through hole pin header THT 1x08 2.54mm single row")
  (fp_text reference REF** (at 0 -2.33) (layer F.SilkS))
  (fp_text value " " (at 1 0) (layer F.Fab))
  (fp_text user CSB (at 3 17.78) (layer F.SilkS))
  (fp_text user AD0 (at 3 12.7) (layer F.SilkS))
  (fp_text user NCS (at 3 15.24) (layer F.SilkS))
  (fp_text user SDA (at 3 10.16) (layer F.SilkS))
  (fp_text user SCL (at 3 7.62) (layer F.SilkS))
  (fp_text user GND (at 3 5.08) (layer F.SilkS))
  (fp_text user 3.3V (at 3 2.54) (layer F.SilkS))
  (fp_text user VIN (at 3 0) (layer F.SilkS))
  (pad 8 thru_hole oval (at 0 17.78) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 7 thru_hole oval (at 0 15.24) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 6 thru_hole oval (at 0 12.7) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 5 thru_hole oval (at 0 10.16) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 4 thru_hole oval (at 0 7.62) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 3 thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
