(module G-NIMO-003 (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value DFN_MO-003_TEC (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.02in/0.5mm" (at -4.2926 -0.500126) (layer Cmts.User))
  (fp_text user "0.008in/0.203mm" (at 4.2926 -0.750189) (layer Cmts.User))
  (fp_text user "0.098in/2.489mm" (at 0 -3.6576) (layer Cmts.User))
  (fp_text user "0.024in/0.61mm" (at -1.2446 3.0226) (layer Cmts.User))
  (fp_text user "0.071in/1.803mm" (at 3.6576 0) (layer Cmts.User))
  (fp_text user "0.051in/1.295mm" (at 0 4.2926) (layer Cmts.User))
  (pad 1 smd rect (at -1.2446 -0.750189) (size 0.6096 0.2032) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.2446 -0.250063) (size 0.6096 0.2032) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -1.2446 0.250063) (size 0.6096 0.2032) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -1.2446 0.750189) (size 0.6096 0.2032) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 1.2446 0.750189) (size 0.6096 0.2032) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 1.2446 0.250063) (size 0.6096 0.2032) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 1.2446 -0.250063) (size 0.6096 0.2032) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 1.2446 -0.750189) (size 0.6096 0.2032) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 0 0) (size 1.2954 1.8034) (layers F.Cu F.Paste F.Mask))
)
