(module Connector_PinSocket_2.54mm:PinSocket_1x07_P2.54mm_Vertical (layer F.Cu) (tedit 641182B0)
  (descr "Through hole straight socket strip, 1x07, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
  (tags "Through hole socket strip THT 1x07 2.54mm single row")
  (fp_text reference REF** (at 0 -19.812) (layer F.SilkS))
  (fp_text value " " (at 4.915 38.775 90) (layer F.Fab))
  (fp_text user VCC (at 7.62 22 90) (layer F.SilkS))
  (fp_text user GND (at 5.08 22 90) (layer F.SilkS))
  (fp_text user SCL (at 2.54 22 90) (layer F.SilkS))
  (fp_text user SDA (at 0 22 90) (layer F.SilkS))
  (fp_text user DC (at -2.54 22 90) (layer F.SilkS))
  (fp_text user CS (at -5.08 22 90) (layer F.SilkS))
  (fp_text user RST (at -7.62 22 90) (layer F.SilkS))
  (fp_text user DISPLAY (at 0 0) (layer F.SilkS))
  (pad 1 thru_hole rect (at -7.62 24.91 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at -5.08 24.91 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 3 thru_hole oval (at -2.54 24.91 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 4 thru_hole oval (at 0 24.91 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 5 thru_hole oval (at 2.54 24.91 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 6 thru_hole oval (at 5.08 24.91 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 7 thru_hole oval (at 7.62 24.91 90) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at 9.63 20.84 90) (size 2 2) (drill 2) (layers *.Cu *.Mask))
  (pad "" np_thru_hole circle (at -9.63 20.84 90) (size 2 2) (drill 2) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_1x07_P2.54mm_Vertical.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
