(module GRAVITECH_CON-SOCJ-2155 (layer F.Cu) (tedit 6322938B)
  (fp_text reference REF** (at 0 -5.5626) (layer F.SilkS))
  (fp_text value GRAVITECH_CON-SOCJ-2155 (at 0 6.6294) (layer F.Fab))
  (pad 3 thru_hole oval (at 0 0) (size 2 4) (drill oval 0.8 2.999999) (layers *.Cu *.Mask))
  (pad 1 thru_hole oval (at 6.1 0) (size 2 4) (drill oval 0.8 3) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 3.3 4.6) (size 4 2) (drill oval 2.999999 0.8) (layers *.Cu *.Mask))
)
