(module Package_SO:HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm (layer F.Cu) (tedit 61B0A8AC)
  (descr "HTSOP, 8 Pin (https://media.digikey.com/pdf/Data%20Sheets/Rohm%20PDFs/BD9G341EFJ.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
  (tags "HTSOP SO")
  (attr smd)
  (fp_text reference REF** (at 0 -3.4) (layer F.SilkS))
  (fp_text value HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm (at 0 3.4) (layer F.Fab))
  (fp_text user %R (at 0 0) (layer F.Fab))
  (pad "" smd roundrect (at 0.6 0.8) (size 0.97 1.29) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at 0.6 -0.8) (size 0.97 1.29) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at -0.6 0.8) (size 0.97 1.29) (layers F.Paste) (roundrect_rratio 0.25))
  (pad "" smd roundrect (at -0.6 -0.8) (size 0.97 1.29) (layers F.Paste) (roundrect_rratio 0.25))
  (pad 9 smd rect (at 0 0) (size 2.4 3.2) (layers F.Cu F.Mask))
  (pad 8 smd rect (at 2.65 -1.905) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 2.65 -0.635) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 2.65 0.635) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 2.65 1.905) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -2.65 1.905) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -2.65 0.635) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -2.65 -0.635) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at -2.65 -1.905) (size 1.6 0.6) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/Package_SO.3dshapes/HTSOP-8-1EP_3.9x4.9mm_P1.27mm_EP2.4x3.2mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
