(footprint "HTSOP-J8_ROM" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tags "BD18IA5MEFJ-ME2 ")
  (attr smd)
  (fp_text reference "REF**" (at 0 0 unlocked) (layer F.SilkS))
  (fp_text value HTSOP-J8_ROM (at 0 0 unlocked) (layer F.Fab))
  (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer F.Fab))
  (fp_text user "*" (at -2.921 -3.5306) (layer F.SilkS))
  (fp_text user "*" (at -1.5748 -2.5527) (layer F.Fab))
  (fp_text user "*" (at -2.921 -3.5306 unlocked) (layer "F.SilkS"))
  (fp_text user "*" (at -1.5748 -2.5527 unlocked) (layer "F.Fab"))
  (pad "1" smd rect (at -2.667 -1.905) (size 1.3716 0.4826) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at -2.667 -0.635) (size 1.3716 0.4826) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "3" smd rect (at -2.667 0.635) (size 1.3716 0.4826) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "4" smd rect (at -2.667 1.905) (size 1.3716 0.4826) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "5" smd rect (at 2.667 1.905) (size 1.3716 0.4826) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "6" smd rect (at 2.667 0.635) (size 1.3716 0.4826) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "7" smd rect (at 2.667 -0.635) (size 1.3716 0.4826) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "8" smd rect (at 2.667 -1.905) (size 1.3716 0.4826) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "EPAD" smd rect (at 0 0) (size 2.413 3.2004) (layers "F.Cu" "F.Mask"))
)
