(footprint "IC57_RP2040" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tags "RP2040 ")
  (attr smd)
  (fp_text reference "REF**" (at 0 0 unlocked) (layer F.SilkS))
  (fp_text value IC57_RP2040 (at 0 0 unlocked) (layer F.Fab))
  (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer F.Fab))
  (fp_text user "*" (at -4.540199 -2.8) (layer F.SilkS))
  (fp_text user "*" (at -2.9972 -2.8) (layer F.Fab))
  (fp_text user "*" (at -4.540199 -2.8 unlocked) (layer "F.SilkS"))
  (fp_text user "*" (at -2.9972 -2.8 unlocked) (layer "F.Fab"))
  (pad "1" smd rect (at -3.4512 -2.6 90) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at -3.4512 -2.200001 90) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "3" smd rect (at -3.4512 -1.799999 90) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "4" smd rect (at -3.4512 -1.4 90) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "5" smd rect (at -3.4512 -1.000001 90) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "6" smd rect (at -3.4512 -0.599999 90) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "7" smd rect (at -3.4512 -0.2 90) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "8" smd rect (at -3.4512 0.2 90) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "9" smd rect (at -3.4512 0.599999 90) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "10" smd rect (at -3.4512 1.000001 90) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "11" smd rect (at -3.4512 1.4 90) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "12" smd rect (at -3.4512 1.799999 90) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "13" smd rect (at -3.4512 2.200001 90) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "14" smd rect (at -3.4512 2.6 90) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "15" smd rect (at -2.6 3.4512) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "16" smd rect (at -2.200001 3.4512) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "17" smd rect (at -1.799999 3.4512) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "18" smd rect (at -1.4 3.4512) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "19" smd rect (at -1.000001 3.4512) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "20" smd rect (at -0.599999 3.4512) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "21" smd rect (at -0.2 3.4512) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "22" smd rect (at 0.2 3.4512) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "23" smd rect (at 0.599999 3.4512) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "24" smd rect (at 1.000001 3.4512) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "25" smd rect (at 1.4 3.4512) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "26" smd rect (at 1.799999 3.4512) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "27" smd rect (at 2.200001 3.4512) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "28" smd rect (at 2.6 3.4512) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "29" smd rect (at 3.4512 2.6 90) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "30" smd rect (at 3.4512 2.200001 90) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "31" smd rect (at 3.4512 1.799999 90) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "32" smd rect (at 3.4512 1.4 90) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "33" smd rect (at 3.4512 1.000001 90) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "34" smd rect (at 3.4512 0.599999 90) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "35" smd rect (at 3.4512 0.2 90) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "36" smd rect (at 3.4512 -0.2 90) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "37" smd rect (at 3.4512 -0.599999 90) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "38" smd rect (at 3.4512 -1.000001 90) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "39" smd rect (at 3.4512 -1.4 90) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "40" smd rect (at 3.4512 -1.799999 90) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "41" smd rect (at 3.4512 -2.200001 90) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "42" smd rect (at 3.4512 -2.6 90) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "43" smd rect (at 2.6 -3.4512) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "44" smd rect (at 2.200001 -3.4512) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "45" smd rect (at 1.799999 -3.4512) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "46" smd rect (at 1.4 -3.4512) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "47" smd rect (at 1.000001 -3.4512) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "48" smd rect (at 0.599999 -3.4512) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "49" smd rect (at 0.2 -3.4512) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "50" smd rect (at -0.2 -3.4512) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "51" smd rect (at -0.599999 -3.4512) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "52" smd rect (at -1.000001 -3.4512) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "53" smd rect (at -1.4 -3.4512) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "54" smd rect (at -1.799999 -3.4512) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "55" smd rect (at -2.200001 -3.4512) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "56" smd rect (at -2.6 -3.4512) (size 0.1786 0.907999) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "57" smd rect (at 0 0) (size 3.2004 3.2004) (layers "F.Cu" "F.Mask"))
)
