(footprint "IFX-PG-TDSON-8-66-V"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "Original name IFX-PG-TDSON-8-66-V\n\nMax Component Height - 1.20mm")
	(property "Reference" "U$1"
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Value" "Comment"
		(at 0.5 0.5 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(fp_text user "Designator"
		(at -4.5 -3.5 0)
		(layer "F.SilkS")
	)
	(fp_text user "${REFERENCE}"
		(at 0.25 0 0)
		(unlocked yes)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -2.863125 -1.905)
		(size 0.925 0.5)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "2" smd rect
		(at -2.863125 -0.635)
		(size 0.925 0.5)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "3" smd rect
		(at -2.863125 0.635)
		(size 0.925 0.5)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "4" smd rect
		(at -2.863125 1.905)
		(size 0.925 0.5)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "5" smd rect
		(at 2.863125 1.905 180)
		(size 0.925 0.6)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "6" smd rect
		(at 2.863125 0.635 180)
		(size 0.925 0.6)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "7" smd rect
		(at 2.863125 -0.635 180)
		(size 0.925 0.6)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
	(pad "8" smd rect
		(at 2.863125 -1.905 180)
		(size 0.925 0.6)
		(layers "F.Cu" "F.Mask")
		(solder_mask_margin 0.1016)
		(thermal_bridge_angle 0)
	)
)