(module IRFP064 (layer F.Cu)
  (fp_text reference REF** (at 5.440001 0.055) (layer F.SilkS))
  (fp_text value TO_P064_VIS (at 5.440001 0.055) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.062in/1.575mm" (at 0 -4.3265) (layer Cmts.User))
  (fp_text user "0.062in/1.575mm" (at 10.880001 4.4365) (layer Cmts.User))
  (fp_text user "TAB" (at 5.440001 -2.5485) (layer F.Fab))
  (pad 1 thru_hole circle (at 0 0) (size 1.5748 1.5748) (drill 1.3208) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 5.440001 0) (size 1.5748 1.5748) (drill 1.3208) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 10.880001 0) (size 1.5748 1.5748) (drill 1.3208) (layers *.Cu *.Mask))
)
