(footprint "Infineon_PG-HSOF-8-1"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "HSOF-8-1 [TOLL] power MOSFET (http://www.infineon.com/cms/en/product/packages/PG-HSOF/PG-HSOF-8-1/)")
	(tags "mosfet hsof toll")
	(property "Reference" "REF**"
		(at 0 -6 0)
		(layer "F.SilkS")
	)
	(property "Value" "Infineon_PG-HSOF-8-1"
		(at 0 6 0)
		(layer "F.Fab")
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "" smd rect
		(at -5.25 -4.2)
		(size 2.6 0.7)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -5.25 -3)
		(size 2.6 0.7)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -5.25 -1.8)
		(size 2.6 0.7)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -5.25 -0.6)
		(size 2.6 0.7)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -5.25 0.6)
		(size 2.6 0.7)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -5.25 1.8)
		(size 2.6 0.7)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -5.25 3)
		(size 2.6 0.7)
		(layers "F.Paste")
	)
	(pad "" smd rect
		(at -5.25 4.2)
		(size 2.6 0.7)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at -0.07 -4.2)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at -0.07 -3)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at -0.07 -1.8)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at -0.07 -0.6)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at -0.07 0.6)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at -0.07 1.8)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at -0.07 3)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at -0.07 4.2)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 1.13 -4.2)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 1.13 -3)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 1.13 -1.8)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 1.13 -0.6)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 1.13 0.6)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 1.13 1.8)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 1.13 3)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 1.13 4.2)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 2.33 -3)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 2.33 -1.8)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 2.33 -0.6)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 2.33 0.6)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 2.33 1.8)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 2.33 3)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 3.53 -3)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 3.53 -1.8)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 3.53 -0.6)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 3.53 0.6)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 3.53 1.8)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 3.53 3)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 4.73 -3)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 4.73 -1.8)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 4.73 -0.6)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 4.73 0.6)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 4.73 1.8)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 4.73 3)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 5.93 -4.2)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 5.93 -3)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 5.93 -1.8)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 5.93 -0.6)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 5.93 0.6)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 5.93 1.8)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 5.93 3)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "" smd circle
		(at 5.93 4.2)
		(size 1 1)
		(layers "F.Paste")
	)
	(pad "1" smd rect
		(at -5.25 -4.2)
		(size 2.8 0.8)
		(layers "F.Cu" "F.Mask")
	)
	(pad "2" smd custom
		(at -4.25 0.6)
		(size 0.8 8)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy -0.4 -3.2) (xy -2.4 -3.2) (xy -2.4 -4) (xy -0.4 -4)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -0.4 -2) (xy -2.4 -2) (xy -2.4 -2.8) (xy -0.4 -2.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -0.4 -0.8) (xy -2.4 -0.8) (xy -2.4 -1.6) (xy -0.4 -1.6)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -0.4 0.4) (xy -2.4 0.4) (xy -2.4 -0.4) (xy -0.4 -0.4)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -0.4 1.6) (xy -2.4 1.6) (xy -2.4 0.8) (xy -0.4 0.8)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -0.4 2.8) (xy -2.4 2.8) (xy -2.4 2) (xy -0.4 2)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -0.4 4) (xy -2.4 4) (xy -2.4 3.2) (xy -0.4 3.2)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(pad "3" smd custom
		(at 3.8 0)
		(size 2.9 8.7)
		(layers "F.Cu" "F.Mask")
		(zone_connect 2)
		(thermal_bridge_angle 45)
		(options
			(clearance outline)
			(anchor rect)
		)
		(primitives
			(gr_poly
				(pts
					(xy 2.85 5.05) (xy 1.45 5.05) (xy 1.45 -5.05) (xy 2.85 -5.05)
				)
				(width 0)
				(fill yes)
			)
			(gr_poly
				(pts
					(xy -1.45 4.85) (xy -5.15 4.85) (xy -5.15 -4.85) (xy -1.45 -4.85)
				)
				(width 0)
				(fill yes)
			)
		)
	)
	(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/Infineon_PG-HSOF-8-1.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)