(module J104D2C5VDC.20S (layer F.Cu)
  (fp_text reference REF** (at 3.81 8.89) (layer F.SilkS))
  (fp_text value RELAY8_J104D2C5VDC.20S_CRS (at 3.81 8.89) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "*" (at 0 -3.386667) (layer F.Fab))
  (fp_text user "*" (at 0 -5.926666) (layer F.SilkS))
  (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 0 7.62) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 0 12.7) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 0 17.78) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 7.62 17.78) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at 7.62 12.7) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
  (pad 7 thru_hole circle (at 7.62 7.62) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
  (pad 8 thru_hole circle (at 7.62 0) (size 1.524 1.524) (drill 1.016) (layers *.Cu *.Mask))
)
