(module Connector_JST:JST_PH_B7B-PH-SM4-TB_1x07-1MP_P2.00mm_Vertical (layer F.Cu) (tedit 63652749)
  (descr "JST PH series connector, B7B-PH-SM4-TB (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
  (tags "connector JST PH side entry")
  (attr smd)
  (fp_text reference REF** (at 0 -5.45) (layer F.SilkS))
  (fp_text value JST_PH_B7B-PH-SM4-TB_1x07-1MP_P2.00mm_Vertical (at 0 4.45) (layer F.Fab))
  (pad MP smd roundrect (at 8.4 -1.75) (size 1.6 3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625))
  (pad MP smd roundrect (at -8.4 -1.75) (size 1.6 3) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.15625))
  (pad 7 smd roundrect (at 6 0.5) (size 1 5.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 6 smd roundrect (at 4 0.5) (size 1 5.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 5 smd roundrect (at 2 0.5) (size 1 5.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 4 smd roundrect (at 0 0.5) (size 1 5.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 3 smd roundrect (at -2 0.5) (size 1 5.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 2 smd roundrect (at -4 0.5) (size 1 5.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (pad 1 smd roundrect (at -6 0.5) (size 1 5.5) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.25))
  (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_B7B-PH-SM4-TB_1x07-1MP_P2.00mm_Vertical.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
