(module Connector_JST:JST_PH_S6B-PH-K_1x06_P2.00mm_Horizontal (layer F.Cu) (tedit 5B7745C6)
  (descr "JST PH series connector, S6B-PH-K (http://www.jst-mfg.com/product/pdf/eng/ePH.pdf), generated with kicad-footprint-generator")
  (tags "connector JST PH top entry")
  (fp_text reference REF** (at 5 -2.55) (layer F.SilkS))
  (fp_text value JST_PH_S6B-PH-K_1x06_P2.00mm_Horizontal (at 5 7.45) (layer F.Fab))
  (fp_text user %R (at 5 2.5) (layer F.Fab))
  (pad 6 thru_hole oval (at 10 0) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask))
  (pad 5 thru_hole oval (at 8 0) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask))
  (pad 4 thru_hole oval (at 6 0) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask))
  (pad 3 thru_hole oval (at 4 0) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at 2 0) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask))
  (pad 1 thru_hole roundrect (at 0 0) (size 1.2 1.75) (drill 0.75) (layers *.Cu *.Mask) (roundrect_rratio 0.208333))
  (model ${KISYS3DMOD}/Connector_JST.3dshapes/JST_PH_S6B-PH-K_1x06_P2.00mm_Horizontal.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
