(module Connector_Audio:Jack_3.5mm_CUI_SJ-3523-SMT_Horizontal (layer F.Cu) (tedit 625E7AD9)
  (descr "3.5 mm, Stereo, Right Angle, Surface Mount (SMT), Audio Jack Connector (https://www.cui.com/product/resource/sj-352x-smt-series.pdf)")
  (tags "3.5mm audio cui horizontal jack stereo")
  (attr smd)
  (fp_text reference REF** (at 0 -9.9) (layer F.SilkS))
  (fp_text value Jack_3.5mm_CUI_SJ-3523-SMT_Horizontal (at 0 10.35) (layer F.Fab))
  (pad "" thru_hole circle (at 0 4.5) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
  (pad "" thru_hole circle (at 0 -2.5) (size 1.7 1.7) (drill 1.7) (layers *.Cu *.Mask))
  (pad T smd rect (at -3.7 5.8) (size 2.8 2.8) (layers F.Cu F.Paste F.Mask))
  (pad S smd rect (at -3.7 -3.6) (size 2.8 2.2) (layers F.Cu F.Paste F.Mask))
  (pad R smd rect (at 3.7 -1.6) (size 2.8 2.2) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/Connector_Audio.3dshapes/Jack_3.5mm_CUI_SJ-3523-SMT_Horizontal.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
