(module Jack_3.5mm_QingPu_WQP-PJ301BM_Vertical (layer F.Cu) (tedit 60E99263)
  (fp_text reference REF** (at -2.6 -6.4) (layer F.SilkS))
  (fp_text value PJ301BM (at 3.7 -6.4) (layer F.Fab))
  (pad T thru_hole oval (at 0 -4.8) (size 4 2) (drill oval 2.5 0.5) (layers *.Cu *.Mask))
  (pad TN thru_hole oval (at 0 3.3) (size 4 2) (drill oval 2.5 0.5) (layers *.Cu *.Mask))
  (pad S2 thru_hole oval (at -4.7 0.6 90) (size 4.5 3) (drill oval 2.5 1) (layers *.Cu *.Mask))
  (pad S1 thru_hole oval (at 4.7 0.6 90) (size 3.8 3) (drill oval 1.8 1) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/AudioJacks.3dshapes/PJ301BM.step
    (offset (xyz 0 0 2))
    (scale (xyz -1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model ${KISYS3DMOD}/AudioJacks.3dshapes/PJ301BM_Hex_nut.step
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
  (model ${KISYS3DMOD}/AudioJacks.3dshapes/PJ301BM_Knurl_nut.step
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
