(module SM141K04LV-Solar-Cell-Footprint (layer F.Cu) (tedit 63D80343)
  (descr "CP, Axial series, Axial, Horizontal, pin pitch=15mm, , length*diameter=10*6mm^2, Electrolytic Capacitor, , http://www.vishay.com/docs/28325/021asm.pdf")
  (tags "CP Axial series Axial Horizontal pin pitch 15mm  length 10mm diameter 6mm Electrolytic Capacitor")
  (fp_text reference REF** (at 0 -2) (layer F.SilkS))
  (fp_text value "Solar Cell" (at 0 10 270) (layer F.Fab))
  (pad 2 smd rect (at 0 20 270) (size 2.5 6) (layers F.Cu F.Paste F.Mask))
  (pad 1 smd rect (at 0 0 270) (size 2.5 6) (layers F.Cu F.Paste F.Mask))
  (model ${KISYS3DMOD}/Capacitor_THT.3dshapes/CP_Axial_L10.0mm_D6.0mm_P15.00mm_Horizontal.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
