(module QFN56_8X8MC_MCH (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value QFN56_8X8MC_MCH (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "*" (at -5.0165 -3.556) (layer F.SilkS))
  (fp_text user "*" (at -3.5687 -3.556) (layer F.Fab))
  (fp_text user "0.02in/0.508mm" (at -6.0071 -3.048) (layer Cmts.User))
  (fp_text user "0.032in/0.813mm" (at -3.9751 -7.0231) (layer Cmts.User))
  (fp_text user "0.01in/0.254mm" (at -7.0231 3.9751) (layer Cmts.User))
  (fp_text user "0.313in/7.95mm" (at 0 9.5631) (layer Cmts.User))
  (fp_text user "0.313in/7.95mm" (at 9.5631 .635) (layer Cmts.User))
  (fp_text user "0.236in/5.994mm" (at 0 6.0452) (layer Cmts.User))
  (fp_text user "0.236in/5.994mm" (at 6.0452 -.635) (layer Cmts.User))
  (fp_text user "*" (at -5.0165 -3.556) (layer F.SilkS))
  (fp_text user "*" (at -3.5687 -3.556) (layer F.Fab))
  (pad 1 smd rect (at -3.9751 -3.302 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -3.9751 -2.794 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -3.9751 -2.286 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -3.9751 -1.778 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -3.9751 -1.27 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -3.9751 -.762 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at -3.9751 -.254 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at -3.9751 .254 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at -3.9751 .762 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at -3.9751 1.27 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at -3.9751 1.778 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at -3.9751 2.286 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at -3.9751 2.794 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd rect (at -3.9751 3.302 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd rect (at -3.302 3.9751) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd rect (at -2.794 3.9751) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 17 smd rect (at -2.286 3.9751) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 18 smd rect (at -1.778 3.9751) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 19 smd rect (at -1.27 3.9751) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 20 smd rect (at -.762 3.9751) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 21 smd rect (at -.254 3.9751) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 22 smd rect (at .254 3.9751) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 23 smd rect (at .762 3.9751) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 24 smd rect (at 1.27 3.9751) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 25 smd rect (at 1.778 3.9751) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 26 smd rect (at 2.286 3.9751) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 27 smd rect (at 2.794 3.9751) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 28 smd rect (at 3.302 3.9751) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 29 smd rect (at 3.9751 3.302 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 30 smd rect (at 3.9751 2.794 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 31 smd rect (at 3.9751 2.286 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 32 smd rect (at 3.9751 1.778 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 33 smd rect (at 3.9751 1.27 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 34 smd rect (at 3.9751 .762 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 35 smd rect (at 3.9751 .254 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 36 smd rect (at 3.9751 -.254 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 37 smd rect (at 3.9751 -.762 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 38 smd rect (at 3.9751 -1.27 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 39 smd rect (at 3.9751 -1.778 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 40 smd rect (at 3.9751 -2.286 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 41 smd rect (at 3.9751 -2.794 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 42 smd rect (at 3.9751 -3.302 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 43 smd rect (at 3.302 -3.9751) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 44 smd rect (at 2.794 -3.9751) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 45 smd rect (at 2.286 -3.9751) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 46 smd rect (at 1.778 -3.9751) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 47 smd rect (at 1.27 -3.9751) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 48 smd rect (at .762 -3.9751) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 49 smd rect (at .254 -3.9751) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 50 smd rect (at -.254 -3.9751) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 51 smd rect (at -.762 -3.9751) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 52 smd rect (at -1.27 -3.9751) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 53 smd rect (at -1.778 -3.9751) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 54 smd rect (at -2.286 -3.9751) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 55 smd rect (at -2.794 -3.9751) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 56 smd rect (at -3.302 -3.9751) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 57 smd rect (at 0 0) (size 5.9944 5.9944) (layers F.Cu ))
)
