(module LDS-SMHTA304RISITR (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value LDS-SMHTA304RISITR_LUM (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.059in/1.5mm" (at -8.798 -2.25) (layer Cmts.User))
  (fp_text user "0.453in/11.5mm" (at 0 6.8199) (layer Cmts.User))
  (fp_text user "0.14in/3.556mm" (at -5.75 -6.8199) (layer Cmts.User))
  (fp_text user "0.049in/1.245mm" (at 8.798 -3) (layer Cmts.User))
  (pad 1 smd rect (at -5.749999 -3.000002) (size 3.556 1.2446) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -5.749999 -1.5) (size 3.556 1.2446) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -5.749999 0) (size 3.556 1.2446) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -5.749999 1.5) (size 3.556 1.2446) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -5.749999 2.999999) (size 3.556 1.2446) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 5.749999 3.000002) (size 3.556 1.2446) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 5.749999 1.5) (size 3.556 1.2446) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 5.749999 0) (size 3.556 1.2446) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 5.749999 -1.5) (size 3.556 1.2446) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at 5.749999 -2.999999) (size 3.556 1.2446) (layers F.Cu F.Paste F.Mask))
)
