(module LED_0805_2012Metric (layer F.Cu) (tedit 5F68FEF1)
  (descr "LED SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
  (tags LED)
  (attr smd)
  (fp_text reference REF** (at 0 -1.65) (layer F.SilkS))
  (fp_text value LED_0805_2012Metric (at 0 1.65) (layer F.Fab))
  (pad 1 smd rect (at -0.9375 0) (size 0.975 1.4) (layers F.Cu F.Mask F.Paste))
  (pad 2 smd rect (at 0.9375 0) (size 0.975 1.4) (layers F.Cu F.Mask F.Paste))
  (fp_text user %R (at 0 0) (layer F.Fab))
  (model ${KISYS3DMOD}/LED_SMD.3dshapes/LED_0805_2012Metric.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)