(module LFOCXO065520BULK (layer F.Cu)
  (fp_text reference REF** (at 25.000001 24.253299) (layer F.SilkS))
  (fp_text value RLA14_IQCM-100_IQD (at 25.000001 24.253299) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "*" (at 0 -3.999999) (layer F.Fab))
  (fp_text user "*" (at 0 -21) (layer F.SilkS))
  (pad 1 thru_hole circle (at 0 0) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 0 6.000001) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 0 24.000003) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 0 30.000004) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 0 36.000004) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
  (pad 6 thru_hole circle (at 0 42.000005) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
  (pad 7 thru_hole circle (at 0 48.000006) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
  (pad 8 thru_hole circle (at 50.000002 48.000006) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
  (pad 9 thru_hole circle (at 50.000002 42.000005) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
  (pad 10 thru_hole circle (at 50.000002 36.000004) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
  (pad 11 thru_hole circle (at 50.000002 30.000004) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
  (pad 12 thru_hole circle (at 50.000002 24.000003) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
  (pad 13 thru_hole circle (at 50.000002 6.000001) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
  (pad 14 thru_hole circle (at 50.000002 0) (size 1.524 1.524) (drill 0.9652) (layers *.Cu *.Mask))
)
