(footprint "LGA-28_5.2x3.8mm_P0.5mm"
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(layer "F.Cu")
	(descr "LGA 28 5.2x3.8mm Pitch 0.5mm")
	(tags "LGA 28 5.2x3.8mm Pitch 0.5mm")
	(property "Reference" "REF**"
		(at 0 -3.25 0)
		(layer "F.SilkS")
	)
	(property "Value" "LGA-28_5.2x3.8mm_P0.5mm"
		(at 0 3.3 0)
		(layer "F.Fab")
	)
	(property "Footprint" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Datasheet" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(property "Description" ""
		(at 0 0 0)
		(unlocked yes)
		(layer "F.Fab")
		(hide yes)
	)
	(attr smd)
	(fp_text user "${REFERENCE}"
		(at 0 0 0)
		(layer "F.Fab")
	)
	(pad "1" smd rect
		(at -2.25 -1.6625)
		(size 0.254 0.675)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "2" smd rect
		(at -2.3875 -0.75 90)
		(size 0.254 0.675)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "3" smd rect
		(at -2.3875 -0.25 90)
		(size 0.254 0.675)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "4" smd rect
		(at -2.3875 0.25 90)
		(size 0.254 0.675)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "5" smd rect
		(at -2.3875 0.75 90)
		(size 0.254 0.675)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "6" smd rect
		(at -2.25 1.6625)
		(size 0.254 0.675)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "7" smd rect
		(at -1.75 1.6625)
		(size 0.254 0.675)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "8" smd rect
		(at -1.25 1.6625)
		(size 0.254 0.675)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "9" smd rect
		(at -0.75 1.6625)
		(size 0.254 0.675)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "10" smd rect
		(at -0.25 1.6625)
		(size 0.254 0.675)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "11" smd rect
		(at 0.25 1.6625)
		(size 0.254 0.675)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "12" smd rect
		(at 0.75 1.6625)
		(size 0.254 0.675)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "13" smd rect
		(at 1.25 1.6625)
		(size 0.254 0.675)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "14" smd rect
		(at 1.75 1.6625)
		(size 0.254 0.675)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "15" smd rect
		(at 2.25 1.6625)
		(size 0.254 0.675)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "16" smd rect
		(at 2.3875 0.75 90)
		(size 0.254 0.675)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "17" smd rect
		(at 2.3875 0.25 90)
		(size 0.254 0.675)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "18" smd rect
		(at 2.3875 -0.25 90)
		(size 0.254 0.675)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "19" smd rect
		(at 2.3875 -0.75 90)
		(size 0.254 0.675)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "20" smd rect
		(at 2.25 -1.6625)
		(size 0.254 0.675)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "21" smd rect
		(at 1.75 -1.6625)
		(size 0.254 0.675)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "22" smd rect
		(at 1.25 -1.6625)
		(size 0.254 0.675)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "23" smd rect
		(at 0.75 -1.6625)
		(size 0.254 0.675)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "24" smd rect
		(at 0.25 -1.6625)
		(size 0.254 0.675)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "25" smd rect
		(at -0.25 -1.6625)
		(size 0.254 0.675)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "26" smd rect
		(at -0.75 -1.6625)
		(size 0.254 0.675)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "27" smd rect
		(at -1.25 -1.6625)
		(size 0.254 0.675)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(pad "28" smd rect
		(at -1.75 -1.6625)
		(size 0.254 0.675)
		(layers "F.Cu" "F.Paste" "F.Mask")
	)
	(model "${KICAD8_3DMODEL_DIR}/Package_LGA.3dshapes/LGA-28_5.2x3.8mm_P0.5mm.wrl"
		(offset
			(xyz 0 0 0)
		)
		(scale
			(xyz 1 1 1)
		)
		(rotate
			(xyz 0 0 0)
		)
	)
)