(footprint "LGA12_STM" (version 20211014) (generator pcbnew)
  (layer "F.Cu")
  (tags "VL53L4CDV0DH/1 ")
  (attr smd)
  (fp_text reference "REF**" (at 0 0 unlocked) (layer F.SilkS))
  (fp_text value LGA12_STM (at 0 0 unlocked) (layer F.Fab))
  (fp_text user "${REFERENCE}" (at 0 0 unlocked) (layer F.Fab))
  (fp_text user "*" (at 0.799973 -2.4765) (layer F.SilkS))
  (fp_text user "*" (at 1.27 -1.6) (layer F.Fab))
  (fp_text user "*" (at 0.799973 -2.4765 unlocked) (layer "F.SilkS"))
  (fp_text user "*" (at 1.27 -1.6 unlocked) (layer "F.Fab"))
  (pad "1" smd rect (at 0.799973 -1.599999 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "2" smd rect (at 0.799973 -0.800001 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "3" smd rect (at 0.799973 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "4" smd rect (at 0.799973 0.800001 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "5" smd rect (at 0.799973 1.599999 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "6" smd rect (at 0 1.599946) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "7" smd rect (at -0.799973 1.599999 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "8" smd rect (at -0.799973 0.800001 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "9" smd rect (at -0.799973 0 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "10" smd rect (at -0.799973 -0.800001 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "11" smd rect (at -0.799973 -1.599999 90) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask"))
  (pad "12" smd rect (at 0 -1.599946) (size 0.508 0.508) (layers "F.Cu" "F.Paste" "F.Mask"))
)
