(module Connector_PinHeader_2.54mm:PinHeader_1x01_P2.54mm_Vertical (layer F.Cu) (tedit 655C9031)
  (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
  (tags "Through hole pin header THT 1x01 2.54mm single row")
  (fp_text reference REF** (at 0.254 -3.048) (layer F.SilkS))
  (fp_text user "- OUT +" (at 39.878 8.89 90) (layer F.SilkS))
  (fp_text user "- IN +" (at 0 8.636 90) (layer F.SilkS))
  (pad 3 thru_hole rect (at 39.497 17.145) (size 1.9 1.9) (drill 1.15) (layers *.Cu *.Mask))
  (pad 4 thru_hole rect (at 39.497 0) (size 1.9 1.9) (drill 1.15) (layers *.Cu *.Mask))
  (pad 2 thru_hole rect (at 0 17.145) (size 1.9 1.9) (drill 1.15) (layers *.Cu *.Mask))
  (pad 1 thru_hole rect (at 0 0) (size 1.9 1.9) (drill 1.15) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x01_P2.54mm_Vertical.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
