(module LSM0805543V (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value LED_LSM0805_2p0x1p25x0p8_VCC (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.049in/1.245mm" (at 4.0513 0) (layer Cmts.User))
  (fp_text user "0.107in/2.718mm" (at 0 -3.6703) (layer Cmts.User))
  (fp_text user "0.047in/1.194mm" (at 0 3.6703) (layer Cmts.User))
  (pad 1 smd rect (at -0.9779 0) (size 0.762 1.2446) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at 0.9779 0) (size 0.762 1.2446) (layers F.Cu F.Paste F.Mask))
)
