(module LSM6DSOTR (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value LGA-14L_2P5X3X0P86_STM (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.02in/0.5mm" (at -3.2258 -0.5) (layer Cmts.User))
  (fp_text user "0.019in/0.475mm" (at -1.2103 -4.0043) (layer Cmts.User))
  (fp_text user "0.01in/0.25mm" (at -4.2583 0.9563) (layer Cmts.User))
  (fp_text user "0.095in/2.421mm" (at 0 6.5443) (layer Cmts.User))
  (fp_text user "0.075in/1.913mm" (at 6.7983 0.635) (layer Cmts.User))
  (fp_text user "*" (at -2.0828 -1) (layer F.SilkS))
  (fp_text user "*" (at -0.9728 -1) (layer F.Fab))
  (pad 1 smd rect (at -1.2103 -0.750001 90) (size 0.351536 0.57658) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.2103 -0.25 90) (size 0.351536 0.57658) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -1.2103 0.25 90) (size 0.351536 0.57658) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -1.2103 0.750001 90) (size 0.351536 0.57658) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -0.499999 0.9563) (size 0.351536 0.57658) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 0 0.9563) (size 0.351536 0.57658) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 0.499999 0.9563) (size 0.351536 0.57658) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 1.2103 0.750001 90) (size 0.351536 0.57658) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at 1.2103 0.25 90) (size 0.351536 0.57658) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at 1.2103 -0.25 90) (size 0.351536 0.57658) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at 1.2103 -0.750001 90) (size 0.351536 0.57658) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at 0.499999 -0.9563) (size 0.351536 0.57658) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at 0 -0.9563) (size 0.351536 0.57658) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd rect (at -0.499999 -0.9563) (size 0.351536 0.57658) (layers F.Cu F.Paste F.Mask))
)
