(module LTC2954CTS8-2-TRMPBF (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value TSOT-23_TS8_LIT (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.026in/0.65mm" (at -4.36245 -0.65) (layer Cmts.User))
  (fp_text user "0.016in/0.406mm" (at 4.36245 -0.975) (layer Cmts.User))
  (fp_text user "0.104in/2.629mm" (at 0 -3.8608) (layer Cmts.User))
  (fp_text user "0.034in/0.876mm" (at -1.31445 3.8608) (layer Cmts.User))
  (fp_text user "*" (at -1.56845 -2.5244) (layer F.SilkS))
  (fp_text user "*" (at -0.4953 -1.3716) (layer F.Fab))
  (pad 1 smd rect (at -1.31445 -0.974999) (size 0.8763 0.4064) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.31445 -0.325001) (size 0.8763 0.4064) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -1.31445 0.325001) (size 0.8763 0.4064) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -1.31445 0.974999) (size 0.8763 0.4064) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 1.31445 0.974999) (size 0.8763 0.4064) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at 1.31445 0.325001) (size 0.8763 0.4064) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at 1.31445 -0.325001) (size 0.8763 0.4064) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at 1.31445 -0.974999) (size 0.8763 0.4064) (layers F.Cu F.Paste F.Mask))
)
