(module UFD_24_ADI (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value UFD_24_ADI (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "*" (at -2.9464 -1.75) (layer F.SilkS))
  (fp_text user "*" (at -1.4986 -1.75) (layer F.Fab))
  (fp_text user "0.02in/0.5mm" (at -3.937 -1.25) (layer Dwgs.User))
  (fp_text user "0.032in/0.813mm" (at -1.905 -5.4483) (layer Dwgs.User))
  (fp_text user "0.01in/0.254mm" (at -4.953 2.4003) (layer Dwgs.User))
  (fp_text user "0.15in/3.81mm" (at 0 7.9883) (layer Dwgs.User))
  (fp_text user "0.189in/4.801mm" (at 7.493 .635) (layer Dwgs.User))
  (fp_text user "0.104in/2.642mm" (at 0 4.8768) (layer Dwgs.User))
  (fp_text user "0.144in/3.658mm" (at 4.3688 -.635) (layer Dwgs.User))
  (fp_text user "*" (at -2.9464 -1.75) (layer F.SilkS))
  (fp_text user "*" (at -1.4986 -1.75) (layer F.Fab))
  (pad 1 smd oval (at -1.905 -1.5 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd oval (at -1.905 -1.000001 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd oval (at -1.905 -.499999 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd oval (at -1.905 0 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd oval (at -1.905 .499999 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd oval (at -1.905 1.000001 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd oval (at -1.905 1.5 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd oval (at -1.000001 2.4003) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd oval (at -.499999 2.4003) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd oval (at 0 2.4003) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd oval (at .499999 2.4003) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd oval (at 1.000001 2.4003) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd oval (at 1.905 1.5 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd oval (at 1.905 1.000001 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd oval (at 1.905 .499999 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd oval (at 1.905 0 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 17 smd oval (at 1.905 -.499999 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 18 smd oval (at 1.905 -1.000001 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 19 smd oval (at 1.905 -1.5 90) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 20 smd oval (at 1.000001 -2.4003) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 21 smd oval (at .499999 -2.4003) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 22 smd oval (at 0 -2.4003) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 23 smd oval (at -.499999 -2.4003) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 24 smd oval (at -1.000001 -2.4003) (size .254 .8128) (layers F.Cu F.Paste F.Mask))
  (pad 25 smd rect (at 0 0) (size 2.6416 3.6576) (layers F.Cu F.Paste F.Mask))
)
