(module LTST-C155KGJRKT (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value SON4_LTST-C155KGJRKT_LTO (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.054in/1.38mm" (at -4.5466 0) (layer Cmts.User))
  (fp_text user "0.033in/0.838mm" (at 4.5466 -0.69) (layer Cmts.User))
  (fp_text user "0.118in/2.997mm" (at 0 -3.7592) (layer Cmts.User))
  (fp_text user "0.032in/0.813mm" (at -1.4986 3.1242) (layer Cmts.User))
  (pad 1 smd rect (at -1.4986 -0.690001) (size 0.8128 0.8382) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.4986 0.690001) (size 0.8128 0.8382) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 1.4986 0.690001) (size 0.8128 0.8382) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 1.4986 -0.690001) (size 0.8128 0.8382) (layers F.Cu F.Paste F.Mask))
)
