(module 21-0113C_MXM (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value 21-0113C_MXM (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "*" (at -1.524 -2.5502) (layer F.SilkS))
  (fp_text user "*" (at -.5588 -1.585) (layer F.Fab))
  (fp_text user "0.1in/2.54mm" (at 0 -5.8166) (layer Cmts.User))
  (fp_text user "0.037in/0.95mm" (at -4.318 -.475) (layer Cmts.User))
  (fp_text user "0.036in/0.914mm" (at -1.1176 3.9116) (layer Cmts.User))
  (fp_text user "*" (at -.5588 -1.585) (layer F.Fab))
  (fp_text user "*" (at -1.524 -2.5502) (layer F.SilkS))
  (pad 1 smd rect (at -1.27 -.950001) (size .9144 .4572) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.27 0) (size .9144 .4572) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -1.27 .950001) (size .9144 .4572) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 1.27 .950001) (size .9144 .4572) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 1.27 -.950001) (size .9144 .4572) (layers F.Cu F.Paste F.Mask))
)
