(module MAX17559ACJ+ (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value 21-0292_MXM (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.031in/0.8mm" (at 7.6581 -2.4) (layer Cmts.User))
  (fp_text user "0.02in/0.508mm" (at 2.8 -7.6454) (layer Cmts.User))
  (fp_text user "0.057in/1.448mm" (at 9.0932 -4.2291) (layer Cmts.User))
  (fp_text user "0.333in/8.458mm" (at -9.0932 0) (layer Cmts.User))
  (fp_text user "0.333in/8.458mm" (at 0 8.9154) (layer Cmts.User))
  (fp_text user "*" (at -5.588 -3.581) (layer F.SilkS))
  (fp_text user "*" (at -3.1242 -3.2) (layer F.Fab))
  (pad 1 smd rect (at -4.2291 -2.799999 90) (size 0.508 1.4478) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -4.2291 -2.000001 90) (size 0.508 1.4478) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -4.2291 -1.2 90) (size 0.508 1.4478) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at -4.2291 -0.399999 90) (size 0.508 1.4478) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at -4.2291 0.399999 90) (size 0.508 1.4478) (layers F.Cu F.Paste F.Mask))
  (pad 6 smd rect (at -4.2291 1.2 90) (size 0.508 1.4478) (layers F.Cu F.Paste F.Mask))
  (pad 7 smd rect (at -4.2291 1.999999 90) (size 0.508 1.4478) (layers F.Cu F.Paste F.Mask))
  (pad 8 smd rect (at -4.2291 2.799999 90) (size 0.508 1.4478) (layers F.Cu F.Paste F.Mask))
  (pad 9 smd rect (at -2.799999 4.2291) (size 0.508 1.4478) (layers F.Cu F.Paste F.Mask))
  (pad 10 smd rect (at -2.000001 4.2291) (size 0.508 1.4478) (layers F.Cu F.Paste F.Mask))
  (pad 11 smd rect (at -1.2 4.2291) (size 0.508 1.4478) (layers F.Cu F.Paste F.Mask))
  (pad 12 smd rect (at -0.399999 4.2291) (size 0.508 1.4478) (layers F.Cu F.Paste F.Mask))
  (pad 13 smd rect (at 0.399999 4.2291) (size 0.508 1.4478) (layers F.Cu F.Paste F.Mask))
  (pad 14 smd rect (at 1.2 4.2291) (size 0.508 1.4478) (layers F.Cu F.Paste F.Mask))
  (pad 15 smd rect (at 1.999999 4.2291) (size 0.508 1.4478) (layers F.Cu F.Paste F.Mask))
  (pad 16 smd rect (at 2.799999 4.2291) (size 0.508 1.4478) (layers F.Cu F.Paste F.Mask))
  (pad 17 smd rect (at 4.2291 2.799999 90) (size 0.508 1.4478) (layers F.Cu F.Paste F.Mask))
  (pad 18 smd rect (at 4.2291 2.000001 90) (size 0.508 1.4478) (layers F.Cu F.Paste F.Mask))
  (pad 19 smd rect (at 4.2291 1.2 90) (size 0.508 1.4478) (layers F.Cu F.Paste F.Mask))
  (pad 20 smd rect (at 4.2291 0.399999 90) (size 0.508 1.4478) (layers F.Cu F.Paste F.Mask))
  (pad 21 smd rect (at 4.2291 -0.399999 90) (size 0.508 1.4478) (layers F.Cu F.Paste F.Mask))
  (pad 22 smd rect (at 4.2291 -1.2 90) (size 0.508 1.4478) (layers F.Cu F.Paste F.Mask))
  (pad 23 smd rect (at 4.2291 -1.999999 90) (size 0.508 1.4478) (layers F.Cu F.Paste F.Mask))
  (pad 24 smd rect (at 4.2291 -2.799999 90) (size 0.508 1.4478) (layers F.Cu F.Paste F.Mask))
  (pad 25 smd rect (at 2.799999 -4.2291) (size 0.508 1.4478) (layers F.Cu F.Paste F.Mask))
  (pad 26 smd rect (at 2.000001 -4.2291) (size 0.508 1.4478) (layers F.Cu F.Paste F.Mask))
  (pad 27 smd rect (at 1.2 -4.2291) (size 0.508 1.4478) (layers F.Cu F.Paste F.Mask))
  (pad 28 smd rect (at 0.399999 -4.2291) (size 0.508 1.4478) (layers F.Cu F.Paste F.Mask))
  (pad 29 smd rect (at -0.399999 -4.2291) (size 0.508 1.4478) (layers F.Cu F.Paste F.Mask))
  (pad 30 smd rect (at -1.2 -4.2291) (size 0.508 1.4478) (layers F.Cu F.Paste F.Mask))
  (pad 31 smd rect (at -1.999999 -4.2291) (size 0.508 1.4478) (layers F.Cu F.Paste F.Mask))
  (pad 32 smd rect (at -2.799999 -4.2291) (size 0.508 1.4478) (layers F.Cu F.Paste F.Mask))
)
