(module MB6S-TP (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value MBS-1_MCC (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2016 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "0.1in/2.54mm" (at -6.02615 0) (layer Cmts.User))
  (fp_text user "0.033in/0.838mm" (at 6.02615 -1.27) (layer Cmts.User))
  (fp_text user "0.234in/5.956mm" (at 0 -4.8895) (layer Cmts.User))
  (fp_text user "0.07in/1.765mm" (at -2.97815 4.8895) (layer Cmts.User))
  (fp_text user "*" (at -3.23215 -3.2512) (layer F.SilkS))
  (fp_text user "*" (at -1.7145 -2.4003) (layer F.Fab))
  (pad 1 smd rect (at -2.97815 -1.27) (size 1.7653 0.8382) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -2.97815 1.27) (size 1.7653 0.8382) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at 2.97815 1.27) (size 1.7653 0.8382) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 2.97815 -1.27) (size 1.7653 0.8382) (layers F.Cu F.Paste F.Mask))
)
