(module SOT-23-5_M5_MCH (layer F.Cu)
  (fp_text reference REF** (at 0 0) (layer F.SilkS))
  (fp_text value SOT-23-5_M5_MCH (at 0 0) (layer F.SilkS))
  (fp_text user "Copyright 2021 Accelerated Designs. All rights reserved." (at 0 0) (layer Cmts.User))
  (fp_text user "*" (at -1.61925 -2.601) (layer F.SilkS))
  (fp_text user "*" (at -.6223 -1.5088) (layer F.Fab))
  (fp_text user "0in/0mm" (at -4.41325 0) (layer Dwgs.User))
  (fp_text user "0.02in/0.508mm" (at 4.41325 -.95) (layer Dwgs.User))
  (fp_text user "0.108in/2.73mm" (at 0 -3.9243) (layer Dwgs.User))
  (fp_text user "0.038in/0.978mm" (at -1.36525 3.9243) (layer Dwgs.User))
  (fp_text user "*" (at -.6223 -1.5088) (layer F.Fab))
  (fp_text user "*" (at -1.61925 -2.601) (layer F.SilkS))
  (pad 1 smd rect (at -1.36525 -.950001) (size .9779 .508) (layers F.Cu F.Paste F.Mask))
  (pad 2 smd rect (at -1.36525 0) (size .9779 .508) (layers F.Cu F.Paste F.Mask))
  (pad 3 smd rect (at -1.36525 .950001) (size .9779 .508) (layers F.Cu F.Paste F.Mask))
  (pad 4 smd rect (at 1.36525 .950001) (size .9779 .508) (layers F.Cu F.Paste F.Mask))
  (pad 5 smd rect (at 1.36525 -.950001) (size .9779 .508) (layers F.Cu F.Paste F.Mask))
)
